## Starting System

#### Starter Overhaul (cont'd)

4-16

Starter Reassembly The reassembly manner is reverse procedure of the disassembly procedure.

1. Apply grease to the following portions.

- Bearings of gear case, rear cover, centre bracket and pinion shaft.
- Mesh area on the reduction gear.
- Shift lever.
- Sliding portion on the pinion.

1. Make sure without metals from inside yoke when reassembly the yoke.

1. Refer to the tightening torque chart for tighten parts.

a a a