## Exterior Trim

#### Front Grille Replacement

20-44

Rear License Trim Replacement

1. Remove the front bumper.

2. Remove the screws (A) and clips (B) and remove the front grille (C) from the front bumper (D) by pulling it out. Take care not to scratch the front bumper.

Fastener Locations

A : Screw, 2B : Clip, 4

3. Remove the screws, then remove the front grille cover (A) from the front grille (B).

   Fastener Locations

   : Screw, 9

4. Install the grille in the reverse order of removal and replace any damaged clips.

1. On the inside of the trunk lid, remove the nuts (A) and release the clips (B), then remove the rear license trim (C). Take care not to scratch the trunk lid.

Fastener Locations

A : Nut, 3B : Clip, 2

2. Install the trim in the reverse order of removal and replace any damaged clips.