## Exterior Lights

#### Front Fog Lights Replacement

22-117
Front Fog Lights Adjustment

(KH model)

1. Remove the two screws from the front fog light (A).

   FRONT FOG LIGHT: 55 W

2. Disconnect the 2P connector (B) from the fog light.

(KH model)

Before adjusting the fog lights:

- Park the vehicle on a level surface.
- Make sure the tire pressures are correct.
- The driver or someone who weights the same should sit in the driver's seat.

Adjust the fog lights to local requirements by turning the adjuster (A).