## Honda Multi Matic Transmission/CVT

#### Symptom Troubleshooting Index (cont'd)

14-251

Symptom | Probable cause(s) | Notes
Excessive idle vibration in and positions |

1. Intermediate housing assembly worn or damaged
2. Input shaft worn or damaged
3. Flywheel drive plate worn or damaged
4. Flywheel assembly defective
5. Engine out put low

Set idle rpm in gear to the specified idle speed. If still no good, adjust the engine and transmissioNmounts.
Noise from transmission in and positions |

1. Intermediate housing assembly worn or damaged
2. Input shaft worn or damaged
3. Planetary carrier worn or damaged
4. Input shaft needle bearing seized up, worn or damaged
5. Thrust needle bearing on planetary carrier seized up, worn or damaged
6. Thrust washer on planetary carrier seized up, worn or damaged
7. ATF pump worn, binding, or foreign material in ATF pump
8. ATF pump chain or ATF pump sprocket worn or damaged
9. Flywheel assembly defective

Check the needle bearing and thrust washers on the planetary carrier for wear and damage. If the needle bearing or thrust washer is worn or damaged, replace the bearing or washer and adjust the clearance with the thrust shim.
Vibration in all positions |

1. Flywheel drive plate worn or damaged
2. Flywheel assembly defective