## ABS Components

#### DTC Troubleshooting Index

19-60

DTC | Detection Item | Note
11 | Right-front wheel sensor (open/short to body ground/short to power) | (see page 19-70)
12 | Faulty right-front wheel sensor pulse signal | (see page 19-71)
13 | Left-front wheel sensor (open/short to body ground/short to power) | (see page 19-70)
14 | Faulty left-front wheel sensor pulse signal | (see page 19-71)
15 | Right-rear wheel sensor (open/short to body ground/short to power) | (see page 19-70)
16 | Faulty right-rear wheel sensor pulse signal | (see page 19-71)
17 | Left-rear wheel sensor (open/short to body ground/short to power) | (see page 19-70)
18 | Faulty left-rear wheel sensor pulse signal | (see page 19-71)
21 | Continuous operation (chipped pulsar) | (see page 19-72)
31 | Solenoid | (see page 19-73)
32 | Solenoid | (see page 19-73)
33 | Solenoid | (see page 19-73)
34 | Solenoid | (see page 19-73)
35 | Solenoid | (see page 19-73)
36 | Solenoid | (see page 19-73)
37 | Solenoid | (see page 19-73)
38 | Solenoid | (see page 19-73)
51 | Motor lock | (see page 19-73)
52 | Motor stuck off | (see page 19-74)
53 | Motor stuck on | (see page 19-74)
54 | Main relay stuck off | (see page 19-75)
61 | Ignition voltage | (see page 19-75)
81 | CPU (Central Processing Unit) | (see page 19-76)