## Honda Multi Matic Transmission/CVT

#### System Description (cont'd)

14-262

Power Flow (cont'd)

Position (Reverse Range)

- Forward clutch: released
- Reverse brake: engaged
- Start clutch: engaged
- Hydraulic pressure is applied to the reverse brake and the start clutch and the planetary carrier locks with the reverse brake.
- The sun gear drives the pinion gears to rotate and the pinion gears drive the ring gear in the opposite direction from the rotation direction of the sun gear.
- The ring gear drives the drive pulley shaft via the forward clutch drum and drive pulley shaft drives the driven pulley shaft linked by the steel belt.
- The driven pulley shaft drives the secondary drive gear via the start clutch.
- Power is transmitted to the secondary driven gear and final drive gear, which in turn drives the final driven gear.

  1. FLYWHEEL
  2. DRIVE PULLEY SHAFT
  3. STEEL BELT
  4. DRIVE PULLEY
  5. FORWARD CLUTCH
  6. REVERSE BRAKE
  7. PLANETARY CARRIER
  8. PINION GEAR
  9. INPUT SHAFT
  10. SUN GEAR
  11. RING GEAR
  12. DRIVEN PULLEY SHAFT
  13. DRIVEN PULLEY
  14. SECONDARY DRIVE GEAR
  15. SECONDARY DRIVEN GEAR
  16. FINAL DRIVEN GEAR
  17. FINAL DRIVE GEAR
  18. START CLUTCH