## Dashboard

#### Dashboard Side Vent Removal/Installation

20-221

Beverage Holder Removal/Installation

NOTE:

- Take care not to scratch the dashboard.
- Put on gloves to protect your hands.

1. Remove the dashboard (see page 20-223).
2. Remove the steering hanger beam from the dashboard (see page 20-226).
3. Remove the screws, then remove the air duct (A) from the dashboard (B).

   Fastener Locations
   : Screw, 7

4. Remove the screws, then remove the side vent (A).

   Fastener Locations
   : Screw, 4

5. Install the side vent in the reverse order of removal.

NOTE:

- Take care not to scratch the dashboard.
- Put on gloves to protect your hands.

1. Remove the dashboard (see page 20-223).
2. Remove the screws, then remove the beverage holder (A).

   Fastener Locations
   : Screw, 2

3. Install the beverage holder in the reverse order of removal.