## Shafts and Clutches

#### Clutch Reassembly (cont'd)

14-212

4. Install the return spring (A) and spring retainer (B) and position the snap ring (C) on the retainer.

5. Install the special tools on the clutch assembly.

6. Be sure the special tool (A) is adjusted to have full contact with the spring retainer (B) on the clutches.

7. If either end of the special tool is set over an area of the spring retainer which is unsupported by the return spring, the retainer may be damaged.