## Fuel Supply System

#### Low Fuel Indicator Light Test

11-443

1. Do the fuel gauge sending unit test (see page 11-441).

- If the system is OK, go to step 2.
- If the system has any malfunction, repair it.

2. Turn the ignition switch ON (II) with the float at the E (EMPTY) position.

- If the low fuel indicator light is on , go to step 3.
- If the low fuel indicator light is not on, refer to the low fuel indicator Circuit Diagram (see page 22-88) and check the circuit.

3. Lift the float above the LOW position.

- If the low fuel indicator light goes off, the system is OK.
- If the low fuel indicator light is still on, refer to the low fuel indicator Circuit Diagram (see page 22-88) and check the circuit.