## Air Conditioning

#### Evaporator Temperature Sensor Test

21-84

1. Dip the sensor in ice water and measure the resistance between its terminals.

EVAPORATOR TEMPERATURE SENSOR

Terminal side of male terminals

2. Then pour hot water on the sensor and check for a change in resistance.
3. Compare the resistance readings with the specifications shown in the graph; the resistance should be within the specifications.