## Dashboard

#### Passenger's Dashboard Lower Cover Removal/Installation

20-220

Glove Box Removal/Installation

NOTE: Take care not to scratch the dashboard and related parts.

1. Remove the passenger's dashboard lower cover (A).

1. Gently pull down the rear edge to release the clips (B).
2. Pull the cover away to release the pins (C) from the holders (D).

Fastener Locations
B : Clip, 3

2. Install the under cover in the reverse order of removal.

SRS components are located in this area. Review the SRS component locations (see page 23-24) and the precautions and procedures (see page 23-25) in the SRS section before performing repairs or service.

NOTE: Take care not to scratch the dashboard and related parts.

1. Remove the passenger's dashboard lower cover.
2. Remove the bolts securing the glove box (A).

   Fastener Location:
   : Bolt, 2

3. While holding the glove box, release the glove box stop (B) on each side from the dashboard by pushing it inside, then remove the glove box.
4. Install the glove box in the reverse order of removal.