## Automatic Transmission

#### System Description (cont'd)

14-30

Power Flow (cont'd)

Position (7-position)

In position, hydraulic pressure is applied to the 1st clutch and the 1st-hold clutch.

The power flow when accelerating is as follows:

- Hydraulic pressure is applied to the 1st clutch, then the 1st clutch engages the mainshaft 1st gear with the mainshaft.
- The mainshaft 1st gear drives the countershaft 1st gear and the countershaft.
- Power is transmitted to the final drive gear, which in turn drives the final driven gear.

  1. TORQUE CONVERTER
  2. 1ST-HOLD CLUTCH
  3. SUB-SHAFT 1ST GEAR
  4. SUB-SHAFT
  5. MAINSHAFT 1ST GEAR
  6. 1ST CLUTCH
  7. MAINSHAFT
  8. COUNTERSHAFT
  9. ONE-WAY CLUTCH
  10. PARK GEAR
  11. COUNTERSHAFT 1ST GEAR
  12. FINAL DRIVEN GEAR
  13. FINAL DRIVE GEAR