## Seat Belts

#### Rear Seat Belt Replacement (cont'd)

23-10

6. Install the seat belt and buckles in the reverse order of removal and note these items:

- With centre shoulder belt: If the threads on the retractor mounting self-tapping ET screw are worn out, use an oversized self-tapping ET screw made specifically for this application.
- With centre shoulder belt: Check that the retractor locking mechanism functions (see page 23-11).
- Assemble the washers on the centre anchor bolt as shown.
- Before installing the centre anchor bolt, make sure there are no twists or kinks in the centre belt.

Centre anchor bolt construction:

1. WASHER
2. CENTRE ANCHOR BOLT
3. TOOTHED LOCK WASHER
4. CENTRE ANCHOR