## Power Distribution

#### Fuse to Components Index

22-4

Under - dash Fuse/Relay Box

Fuse Number | Amps | Wire Colour | Component(s) or Circuit(s) Protected
1 | 15A | BLK/WHT | Ignition coils
2 | ——— | ——— | Not used
3 | 10A | Fuse/relay box socket | Multiplex control unit (KG model: daytime running lights)
| ——— |
4 | 10A | BLK/ORN | Alternator, Cruise control unit, Cruise main switch, EVAP purge control solenoid valve, Primary HO2S, Secondary HO2S, Vehicle speed sensor, Shift lock relay (KG model: daytime running lights)
5 | 7.5A | Fuse/relay box socket | Multiplex control unit (KG model)
6 | 7.5A | YEL/GRN | Headlight adjuster switch, Headlight adjuster unit, Power window master switch, Sunroof open relay, Sunroof close relay
7 | 20A | GRN | Sunroof motor
8 | 7.5A | Fuse/relay box socket | Optional connector V, Multiplex control unit
YEL/RED | Audio unit, Interlock control unit (KG model: daytime running lights), Key interlock relay (KG model: daytime running lights), Shift lock relay (Except KG model: daytime running lights)
9 | 10A | GRN | OPDS unit
10 | 7.5A | Fuse/relay box socket | Multiplex control unit
YEL | A/T reverse relay, Back-up lights, EPS control unit, Gauge assembly, Keyless receiver unit, Security control unit
11 | 7.5A | BLK/ORN | ABS modulator-control unit
12 | 7.5A | Fuse/relay box socket | Multiplex control unit (KG model: daytime running lights)
13 | 10A | PNK | SRS unit
14 | 10A | Fuse/relay box socket | Optional connector V
BLK/YEL | A/C compressor clutch relay, Blower motor relay, Condenser fan relay, Climate control unit (with auto A/C), Heater control panel (without auto A/C), Power mirror actuator, Power mirror defogger, Radiator fan relay, Rear window defogger relay, Recirculation control motor, Seat heater main relay
15 | 30A | RED/YEL | Headlight washer control unit
16 | 20A | RED/BLK | Driver's seat heater, Passenger's seat heater
17 | 15A | BLK/YEL | Inertia switch, SRS unit
YEL/BLK | ECM, PCM, Fuel pump
18 | 15A | YEL/GRN | Cigarette lighter
19 | 7.5A | YEL/BLK | Turn signal/hazard relay
20 | 20A | Fuse/relay box socket | Multiplex control unit
GRN/BLK | Windshield wiper motor, Windshield washer motor
21 | ——— | ——— | Not used
22 | 20A | GRN/BLK | Front passenger's power window motor
23 | 20A | GRN/WHT | Driver's power window motor
24 | 20A | YEL/RED | Left rear power window motor
25 | 20A | YEL/BLU | Right rear power window motor