## SRS

#### DTC Troubleshooting Index (cont'd)

23-47

DTC | Detection Item | Notes
9-1 | Internal failure of the SRS unit. If intermittent, could mean internal failure of the unit or a faulty indicator light circuit. Refer to Troubleshooting Intermittent Failures (see page 23-38). | (see page 23-85)
9-2 | Internal failure of the SRS unit. If intermittent, could mean internal failure of the power supply (VB line). Refer to Troubleshooting Intermittent Failures (see page 23-38).
9-6 | Faulty left front sensor | (see page 23-88)
9-7 | Faulty right front sensor | (see page 23-91)
10-1 | Seat belt tensioners (and airbag(s)) deployed | (see page 23-85)
10-2 | Left side airbag deployed
10-3 | Seat belt tensioners (and airbag(s)) and left side airbag deployed
10-4 | Right side airbag deployed
10-5 | Seat belt tensioners (and airbag(s)) and front right side airbag deployed
10-6 | Side airbags deployed
10-7 | Seat belt tensioners (and airbag(s)) and side airbags deployed
11-1 | Open or increased resistance in left side airbag inflator | (see page 23-100)
11-3 | Short to another wire or decreased resistance in left side airbag inflator | (see page 23-101)
11-4 | Short to power in left side airbag inflator | (see page 23-103)
11-5 | Short to ground in left side airbag inflator | (see page 23-104)
12-1 | Open or increased resistance in right side airbag inflator | (see page 23-112)
12-3 | Short to another wire or decreased resistance in right side airbag inflator | (see page 23-113)
12-4 | Short to power in right side airbag inflator | (see page 23-115)
12-5 | Short to ground in right side airbag inflator | (see page 23-116)
13-1 | Internal failure of the left side impact sensor | (see page 23-87)
13-2
13-3 | No signal from the left side impact sensor | (see page 23-121)
13-4 | Faulty power supply to the left side impact sensor | (see page 23-122)
14-1 | Internal failure of the right side impact sensor | (see page 23-87)
14-2
14-3 | No signal from the right side impact sensor | (see page 23-127)
14-4 | Faulty power supply to the right side impact sensor | (see page 23-128)