## Exterior Trim

#### Emblem Replacement

20-10

NOTE:

- When removing the emblem, take care not to scratch the body.
- For the front and rear "H" emblem, refer to the '01 Civic Shop Manual, P/N 62S5A00 on this CD (see page 20-257).

1. Clean the body surface with a sponge dampened in alcohol. After cleaning, keep oil, grease and water from getting on the surface.
2. Apply the emblem, where shown.

   1. VTEC EMBLEM

      (For some models)

   2. FRONT "H" EMBLEM
   3. CIVIC EMBLEM

      (KG, KR and KS models)

      or VERSION EMBLEM

      (KE and KY models)

   4. VERSION EMBLEM

      (KE, KG and KR models)

   5. REAR "H" EMBLEM
   6. CIVIC EMBLEM

      (KE and KY models)

      or HONDA EMBLEM

      (For some models)

Unit: mm (in)