## Engine Assembly

#### Engine Installation

5-10

1. Install the accessory brackets and tighten their bolts and nuts to the specified torques.

1. REAR STIFFENER

   (D17A8, D17A9 engines M/T)

2. REAR STIFFENER

   (D17A8, D17A9 engines A/T)

3. P/S PUMP BRACKET
4. ENGINE MOUNT BRACKET
5. A/C COMPRESSOR BRACKET
6. STIFFENER

   (D17A2, D17A5, D17A8, D17A9 engines A/T)

7. FRONT STIFFENER

   (D17A8, D17A9 engines)