## Climate Control

#### Climate Control Unit Removal and Installation

21-153

1. Remove the centre panel (see page 20-78).

2. Remove the dials (A), then remove the self-tapping screws and the climate control unit (B) from the centre panel (C).

3. Install the control unit in the reverse order of removal. After installation, operate the control unit controls to see whether it works properly.
4. Run the self-diagnosis function to confirm that there are no problems in the system (see page 21-104).