## Automatic Transmission

#### DTC Troubleshooting Index

14-9

DTC | Indicator Light | MIL | Detection Item | Page
OBD Scan Tool | PGM Tester | Indicator Light
P0715 | 15-1 | 15 | Blinks | ON | Mainshaft speed sensor | (see page 14-76)
P0720 | 9-1 | 9 | Blinks | ON | Countershaft speed sensor | (see page 14-78)
P0730 | 41-1 | 41 | OFF | ON | Shift control system | (see page 14-79)
P0753 | 7-1 | 7 | Blinks | ON | Shift solenoid valve A | (see page 14-80)
P0758 | 8-1 | 8 | Blinks | ON | Shift solenoid valve B | (see page 14-82)
P1705 | 5-1 | 5 | Blinks | ON | Transmission range switch (short to ground) | (see page 14-84)
P1706 | 6-1 | 6 | OFF | ON | Transmission range switch (open) | (see page 14-87)
P1713 | 21-1 | 21 | OFF | OFF | D3 switch | (see page 14-90)
P1753 | 1-1 | 1 | Blinks | ON | Torque converter clutch solenoid valve | (see page 14-91)
P1768 | 16-1 | 16 | Blinks | ON | A/T clutch pressure control solenoid valve A | (see page 14-93)
P1773 | 23-1 | 23 | Blinks | ON | A/T clutch pressure control solenoid valve B | (see page 14-95)

NOTE: The function of detecting the D3 switch problem is applied to only the 5-door model.