## Doors

#### Rear Door Glass, Quarter Glass and Regulator Replacement (cont'd)

20-21

11. Install the glass and regulator in the reverse order of removal, and note these items:

- Roll the glass up and down to see if it moves freely without binding.
- Make sure that there is no clearance between the glass and glass run channel when the glass is closed.
- Adjust the position of the glass as necessary (see page 20-24).