## Frame Repair Chart

#### Side View (cont'd)

4-21

l | Locate hole o 25 (0.98) | t | For upper arm bracket center o 15 (0.59)
m | For trailing arm o 13 (0.51) | u1, u2 | Locate hole o 13 (0.51)
n | Locate hole o 25 (0.98) | v | For upper arm o 13 (0.51)
o | Locate hole o 20 (0.79) | w | Locate hole o 13 (0.51)
p | Trailing arm centre | x | For rear lower arm centre
q | Rear damper center 73 x 68 (slot) | y | Locate hole o 50 (1.97)
r | For upper arm o 13 (0.51) | z | Locate hole o 20 (0.79)
s | For trailing arm o 13 (0.51)