## Heating

#### DTC Troubleshooting Index (cont'd)

21-7

5-door KE Model

DTC (Recirculation Indication Light Blinks) | Detection Item | Page
7 | An open in the air mix control motor circuit | (see page 21-24)
8 | A short in the air mix control motor circuit | (see page 21-24)
9 | A problem in the air mix control linkage, door or motor | (see page 21-25)
10 | An open or short in the mode control motor circuit | (see page 21-26)
11 | A problem in the mode control linkage, doors or motor | (see page 21-27)
12 | A problem in the blower motor circuit | (see page 21-28)
13 | A problem in the EEPROM in the heater control panel; the control panel must be replaced | (see page 21-51)
14 | An open in the evaporator temperature sensor circuit | (see page 21-31)
15 | A short in the evaporator temperature sensor circuit | (see page 21-32)

In case of multiple problems, the recirculation indicator light will indicate only the DTC with the least number of blinks.