## Fenderwell

#### Rear Strake Replacement

20-261

Fuel Pipe Protector Replacement

For Some Model

1. Remove the screws, then remove the rear strake (A). Take care not to scratch the body.

   Fastener Locations
   : Screw, 2

2. Install the strake in the reverse order of removal.

1. Remove the clips, then remove the fuel pipe protector (A). Take care not to scratch the body.

Fastener Locations
: Clip, 4

2. Install the protector in the reverse order of removal and replace any damaged clips.