## Exterior Trim

#### Emblem Replacement

20-45

NOTE: When removing the emblems, take care not to scratch the body.

1. Clean the body surface with a sponge dampened in alcohol. After cleaning, keep oil, grease and water from getting on the surface.
2. Apply the emblem where shown.

1. HONDA EMBLEM (KG, KB, KR models)/VTEC EMBLEM (KY model)
2. VERSION EMBLEM (KB, KK, KX, KY models)/VTEC EMBLEM (KE, KG, KR model)
3. CIVIC EMBLEM

Unit: mm (in.)