## Interior Trim

#### Trim Removal/Installation - Rear Shelf Area - Fixed Type Rear Seat

20-66

NOTE:

- Put on gloves to protect your hands.
- When prying with a flat-tip screwdriver, wrap it with protective tape to prevent damage.
- Take care not to bend or scratch the trim and panels.

Remove the trim as shown. To remove the rear shelf, remove the rear seat (see page 20-96).

Install the trim in the reverse order of removal, and note these items:

- Replace any damaged clips.
- When installing the rear shelf, slip the rear seat belts through the slits in the rear shelf.
- Make sure the high mount brake light connector is plugged in properly.

  Fastener Locations
  A : Clip, 5 (White) | B : Clip, 11
  1. BODY
  2. HOOK
  3. REAR SHELF
  4. HOOK
  5. REAR PILLAR TRIM
  6. REAR WINDOW DEFOGGER HARNESS
  7. REAR DOOR OPENING TRIM
  8. SLIT
  9. SEAT SIDE TRIM
  10. REAR SEAT BELT
  11. REAR SHELF
  12. HIGH MOUNT BRAKE LIGHT CONNECTOR
  13. REAR SEAT BELT
  14. SLIT
  15. HOOK