## Front Wheelhouse/Damper Housing

#### Removal

3-7

- Cut and remove the wheelhouse upper member, and replace the front wheelhouse.

1. DAMPER HOUSING
2. FRONT DAMPER EXTENSION
3. WHEELHOUSE UPPER MEMBER Reused.
4. FRONT WHEELHOUSE
5. ENGINE MOUNT BRACKET
6. FRONT SIDE FRAME

- Check the front damper extension and damper housing for position and damage. If necessary, remove the wheelhouse upper member and replace the damper housing and front damper extension as an assembly, if possible.

1. DAMPER HOUSING
2. FRONT DAMPER EXTENSION
3. WHEELHOUSE UPPER MEMBER Reused.