## Upper Body Measuring Dimensions

#### Engine Compartment

4-14

Unit: mm (in.)

1. E, e

   Front Damper Mount Hole 11.5 (0.45)

2. G, g

   Hood Hinge Mount Hole 7 (0.3) Forward

3. F, f

   Front Fender Mount Hole 7 (0.3) middle

4. D, d

   Front Bumper Beam Mount Hole 9 (0.35)

5. C, c

   Front Fender Mount Hole 7 (0.3) Forward

6. B, b

   Headlight Mount Hole 7 (0.3)

7. A, a

   Bulkhead Upper Frame Point 15 (0.59)