## Power Distribution

#### Fuse to Component Index

22-8

Under-hood Fuse/Relay Box

Fuse Number | Amps | Wire Colour | Component(s) or Circuit(s) Protected
1 | 30A | BLU/YEL | Condenser fan motor
2 | 15A | WHT/GRN | Dash lights, Front parking lights, Multiplex control unit, License plate lights, Taillights, Taillight relay
3 | 7.5A | WHT/BLU | Ceiling light, Spotlights, Cargo light
4 | 10A | BLU/BLK | A/C compressor clutch
5 | 15A | WHT/BLK | Hazard warning light, Security control unit, Turn signal/hazard relay
6 | 20A | WHT/BLK | Main relay, ECM, Engine glow relay, Water heater relay 1, Water heater relay 2
7 | 15A | WHT/GRN | ABS modulator-control unit, Brake lights, Multiplex control unit, Security horn relay, ECM, Horn
8 | 20A | WHT/GRN | ABS modulator-control unit
9 | 10A | WHT/RED | Audio unit, Data link connector, Gauge assembly, Multiplex control unit, Immobiliser receiver unit, Keyless receiver unit, Security control unit
10 | 40A | WHT/RED | ABS modulator-control unit
11 | 30A | BLK/YEL | Rear window defogger, Noise condenser
12 | 40A | BLU/WHT | Blower motor
13 | 40A | WHT/BLK | Power window motors, Sunroof motor
14 | 40A | WHT/RED | No. 3, 5, 15 and 16 fuses (in the under-dash fuse/relay box)
15 | 15A | RED/YEL | High beam indicator light, Left headlight
16 | 20A | WHT | Multiplex control unit
17 | 15A | RED | Right headlight
18 | 60A | WHT/BLU | EPS control unit
19 | 100A | - | Battery, Power distribution
20 | 50A | WHT | Ignition switch (BAT)

: Spare fuse

a a a