## EPS Components

#### DTC Troubleshooting (cont'd)

17-92

DTC 69: EPS Control Unit Internal Circuit

1. Clear the DTC.
2. Start the engine.
3. Turn the steering wheel from lock-to-lock several time, and wait 10 seconds or more.

Does the EPS indicator come on?

YES - Go to step 4.

NO - The system is OK at this time.

4. Stop the engine, and verify the DTC.

Is DTC 69 indicated?

YES - Check for loose EPS control unit connectors. If necessary, substitute a known-good EPS control unit and recheck.

NO - Perform the appropriate troubleshooting for the code indicated.