## Manual Transmission

#### Countershaft Reassembly (cont'd)

13-39

1. Install the needle bearing.

1. Install the 2nd gear (A) by aligning the synchro cone fingers (B) with the grooves in 2nd gear (C).

1. Support the countershaft (A) on the steel blocks, then install the 3rd gear (B) using the special tool and a press (C).

1. Install the 4th gear (A) using the special tool and a press (B).

1. Install the 5th gear (A) using the special tool and a press (B).

a a a