## Cylinder Head

#### Cam Chain Installation (cont'd)

6-17

1. Install the cam chain on the crankshaft sprocket with the coloured piece (A) aligned with the punch mark (B) on the crankshaft sprocket.

1. Install the cam chain on the VTC actuator and exhaust camshaft sprocket with the punch marks (A) aligned with the two coloured pieces (B).

1. Install the cam chain guide A (A) and tensioner arm (B).

1. Install the auto-tensioner.

a a a