## Power Distribution

#### Fuse to Components Index

22-43

Under-hood Fuse/Relay Box

Fuse Number | Amps | Wire Colour | Component(s) or Circuit(s) Protected
1 | 20A | BLU/YEL | Condenser fan motor
BLU/RED | A/C compressor clutch
2 | 15A | WHT/GRN | Dash lights, Front parking lights, Front side marker lights (KK model), Multiplex control unit (KG model), License plate lights, Taillights, Taillight relay
3 | 7.5A | WHT/BLU | Ceiling light, Spotlights, Trunk light
4 | 20A | BLU/BLK | Radiator fan motor
5 | 10A | WHT/BLK | Hazard warning light (KM model, KP model), Security control unit (KK model: EX, KH model, TR model: 1.6 ES, KG model: 1.6 ES, KN model), Turn signal/hazard relay
6 | 15A | WHT/BLK | CKP sensor, ECM/PCM, Fuel injectors, IAC valve, Immobiliser receiver unit, PGM-FI main relay 1 and 2, TDC sensor
7 | 15A | WHT/GRN | ABS modulator-control unit, Brake lights, Cruise control unit, ECM, Multiplex control unit, PCM, Security horn relay (KK model: EX, KH model, TR model: 1.6 ES, KG model: 1.6 ES, KN model), Security horn (KK model: EX, KH model, TR model: 1.6 ES, KG model: 1.6 ES, KN model), Shift lock solenoid (KH model)
8 | 20A | WHT/GRN | ABS modulator-control unit
9 | 10A | WHT/RED | Audio unit, Data link connector, Gauge assembly, Multiplex control unit, Immobiliser indicator light, Immobiliser receiver unit, Keyless receiver unit, Security control unit (KK model: EX, KH model, TR model: 1.6 ES, KG model: 1.6 ES, KN model)
10 | 40A | WHT/RED | ABS modulator-control unit
11 | 30A | BLK | Rear window defogger
12 | 40A | BLU/WHT | Blower motor
13 | 40A | WHT/BLK | Power window motors, Sunroof motor
14 | 40A | WHT/RED | No. 3, 5, 15 and 16 fuses (in the under-dash fuse/relay box)
15 | 15A | RED/YEL | High beam indicator light, Headlight washer control unit, Left headlight
16 | 20A | WHT | Multiplex control unit
17 | 15A | RED | Right headlight
18 | 60A | WHT/BLU | EPS control unit
19 | 80A | ——— | Battery, Power distribution
20 | 50A*¹ 40A*² | WHT | Ignition switch (BAT)

*¹: KB model, KG model, TR model, KE model

*²: Except KB model, KG model, TR model, KE model

: Spare Fuse