## Transmission Housing

#### Reverse Idler Gear Removal and Installation

14-178

Removal

1. Remove the two bolts securing the reverse idler gear shaft holder, then remove the reverse idler gear shaft holder (A) and needle bearing (B).

2. Remove the reverse idler gear.

Installation

1. Install the reverse idler gear in the transmission housing.

2. Install the needle bearing (A) in the reverse idler gear (B).

3. Install the reverse idler gear shaft holder (C) into the transmission housing, then tighten the bolts.