## Seats

#### Rear Seat Side Bolster Cover Replacement - Folding Type

20-101

1. Remove the seat side bolster (see page 20-95).

2. Release all the hook strips (A), and fold back the seat side bolster cover (B), and release the cover from the hooks (C), to remove it.

3. Install the cover in the reverse order of removal, and to prevent wrinkles, make sure the material is stretched evenly over the pad before securing the hook strips.