## Fuse/Relay Boxes

#### Connector to Fuse/Relay Box Index (cont'd)

22-42

Under-dash Fuse/Relay Box

Socket | Ref. | Terminal | Connects to
A | 4 | 5 | Dashboard wire harness B
B | 6 | 6 | Dashboard wire harness B
C | 2 | 14 | Dashboard wire harness B
D | 3 | 12 | ECM/PCM wire harness
Diode | 27 | ——- |
E | 5 | 13 | ECM/PCM wire harness
F | 28 | 12 | Engine compartment wire harness
G | 9 | 10 | Engine compartment wire harness
H | 7 | 3 | Engine compartment wire harness
I | 29 | 5 | Engine compartment wire harness
J | 30 | 8 | Engine compartment wire harness
K | 13 | 17 | Dashboard wire harness A
L | 14 | 10 | Dashboard wire harness A
M | 12 | 12 | Dashboard wire harness A
N | 11 | 6 | Dashboard wire harness A
O | 16 | 12 | Dashboard wire harness A
P | 8 | 18 | Floor wire harness
Power window relay | 20 | 4 |
Q | 1 | 8 | Floor wire harness
R | 19 | 6 | ECM/PCM wire harness
S | 15 | 2 | Dashboard wire harness B
Starter cut relay | 24 | 4 |
T | 21 | 3 | Service check connector
Taillight relay | 22 | 4 |
Turn signal/hazard relay | 10 | 4 |
U | 23 | 1 | Optional connector
V | 26 | 4 | Optional connector
W | 25 | 2 | Floor wire harness (Memory erase signal connector
X | 17 | 8 | Dashboard wire harness B
Y | 18 | 13 | Dashboard wire harness A