## Automatic Transmission

#### System Description (cont'd)

14-21

Position

Hydraulic pressure is not applied to the clutches. Power is not transmitted to the countershaft. The countershaft is locked by the park pawl interlocking the park gear.

Position

Engine power transmitted from the torque converter drives the mainshaft, but hydraulic pressure is not applied to the clutches. Power is not transmitted to the countershaft. The countershaft 4th gear is engaged with the reverse selector hub and the countershaft by the reverse selector when the shift lever is shifted in position from position. The countershaft reverse gear is engaged when shifted from position.

1. TORQUE CONVERTER
2. 2ND CLUTCH
3. 4TH CLUTCH
4. 1ST-HOLD CLUTCH
5. SUB-SHAFT
6. 1ST CLUTCH
7. MAINSHAFT
8. COUNTERSHAFT
9. PARK GEAR
10. ONE-WAY CLUTCH
11. SERVO VALVE
12. 3RD CLUTCH
13. FINAL DRIVEN GEAR
14. FINAL DRIVE GEAR