## Console

#### Centre Console Rear Cover Replacement

20-74

Centre Console Trim Replacement

NOTE: Take care not to scratch the centre console.

1. Remove the centre console (see page 20-73).
2. Remove the screws, then remove the centre console rear cover (A).

   Fastener Locations
   : Screw, 2

3. Install the cover in the reverse order of removal.

NOTE: Take care not to scratch the centre console.

1. Remove the centre console (see page 20-73).
2. Remove the screws, then remove the centre console trim (A). MT model is shown, AT model is similar.

   Fastener Locations
   : Screw, 4

3. Install the trim in the reverse order of removal.