## Clutch

#### Clutch Master Cylinder Installation (cont'd)

12-5c

10. Install the clutch master cylinder.

11. For the left-side steering vehicles attach the clutch line (A) to the clutch line clip (B).

12. Bleed the clutch hydraulic system.
13. Fill brake fluid up to the MAX line on the reservoir. Push back the diaphragm in the reservoir to the initial condition and after fitting it, attach the cap.

12-5c 12-7 home