## Manual Transmission

#### Transmission Installation (cont'd)

13-14

25. Install the intake air duct (see step 39 on page 5-20).

26. Install the battery. Connect the positive (+) cable first, then the negative (-) cable to the battery.
27. Refill the transmission fluid (see page 13-3).
28. Test-drive the vehicle.
29. Check the clutch operation.
30. Check the transmission for noise and smooth operation.
31. Check the front wheel alignment (see page 18-4).
32. Enter the anti-theft code for the radio, then enter the customer's radio station presets.