## Engine Assembly

#### Engine Installation (cont'd)

5-19

32. Connect the PCM connectors.

RHD models:

LHD models:

33. Install the glove box stops.

34. Install the cruise control cable, then adjust the cable (see page 4-48).
35. Install the throttle cable, then adjust the cable (see page 11-148).
36. Install the brake booster vacuum hose.

RHD models (4-door):

RHD models (5-door):

LHD models: