## Automatic Transmission

#### Interlock System - Reverse Lock System Circuit Troubleshooting (cont'd)

14-74

13. Shift the shift lever to position while pushing the shift lock release.
14. Check for continuity between the No. 2 terminal of the interlock relay connector and body ground when the shift lever is in position and when the shift lever out of to , , or position.

INTERLOCK RELAY CONNECTOR

Wire side of female terminals

Is there continuity when the shift lever in position and no continuity when the shift lever in D.gif, , or position?

YES - Check for loose terminal fit in the interlock control unit connector. If necessary, substitute a known-good interlock control unit and recheck.

NO - Repair open in position wire between the No. 2 terminal of the interlock relay connector and the shift position switch.