## ABS Components

#### DTC Troubleshooting (cont'd)

19-110

DTC 61, 62: FSR +B Voltage

1. Clear the DTC (see page 19-90).
2. Test-drive the vehicle at 6 mph (10 km/h) or more.

Does the ABS indicator come on?

YES - Go to step 3.

NO - The system is OK at this time.

3. Verify the DTC.

Is DTC 61 or 62 indicated?

YES - Check the charging system.

NO - Perform the appropriate troubleshooting for the code.

DTC 71: Different Diameter Tyre

1. Clear the DTC (see page 19-90).
2. Test-drive the vehicle.

Does the ABS indicator come on and is DTC 71 indicated?

YES - Make sure all four tyres are the specified size and are inflated to proper specification.

NO - Intermittent failure; the vehicle is OK at this time.