## Dashboard

#### Driver's Tray Removal/Installation

20-222

Passenger's Tray Removal/Installation

NOTE:

- Take care not to scratch the dashboard.
- Put on gloves to protect your hands.

1. Remove the dashboard (see page 20-223).
2. Remove the beverage holder (see page 20-221).
3. Remove the screws, then remove the driver's tray (A).

   Fastener Locations
   : Screw, 3

4. Install the tray in the reverse order of removal.

NOTE:

- Take care not to scratch the dashboard.
- Put on gloves to protect your hands.

1. Remove the dashboard (see page 20-223).
2. Remove the steering hanger beam from the dashboard (see page 20-226).
3. Remove the air duct (see step 3 on page 20-221).
4. Remove the screws, then remove the passenger's tray (A).

   Fastener Locations
   : Screw, 8

5. Install the tray in the reverse order of removal.