## SRS

#### Connectors

23-53

Connector No. *1 | Wire harness and connector | Terminal | Note *2 | Ref. No.
Male | Female
U1o | Dashboard wire harness B 18P connector |  | O | a | 1
U2o | Floor wire harness 18P connector |  | O | a | 2
U3o | Floor wire harness 8P connector |  | O | a | 3
F1o | Dashboard wire harness B 2P connector |  | O | a | 4
F2o | Floor wire harness 18P connector |  | O |  | 5
F3o | Dashboard wire harness B 17P connector |  | O |  | 6
D1 | D1o | Driver's airbag 2P connector |  | O | ab | 7
D1i | Cable reel 2P connector | O |  | 8
D2 | D2o | Cable reel 4P connector |  | O | a | 8
D2i | Dashboard wire harness B 4P connector | O |  | 7
P1 | P1o | Front passenger's airbag 2P connector |  | O | ab | 10
P1i | Dashboard wire harness B 2P connector | O |  | 9
TL1 | TL1o | Left side seat belt tensioner 2P connector |  | O | ab | 10
TL1i | Floor wire harness 2P connector | O |  | 9
TR1 | TR1o | Right side seat belt tensioner 2P connector |  | O | ab | 10
TR1i | Floor wire harness 2P connector | O |  | 9
T2 | T2o | Floor wire harness 4P connector | O |  | a | 7
T2i | Dashboard wire harness B 4P connector |  | O | 8
SD(L) | SD(L)o | Driver's (Left) side airbag 2P connector | O |  | abc | 11
SD(L)i | Floor wire harness 2P connector |  | O | 12
SP(R) | SP(R)o | Front passenger's (Right) side airbag 2P connector | O |  | abc | 11
SP(R)i | Floor wire harness 2P connector |  | O | 12
FS | FSL1i | Engine compartment wire harness 2P connector |  | O | ac | 13
FSR1i | Engine compartment wire harness 2P connector |  | O | 13
FS2 | FS2o | Engine compartment wire harness 4P connector |  | O | a | 8
FS2i | Dashboard wire harness B 4P connector | O |  | 7
ID(L)I | Floor wire harness 2P connector |  | O | ac | 13
IP(R)I | Floor wire harness 2P connector |  | O |  | 13
O1i | OPDS unit harness 8P connector |  | O |  | 14
C1 | Dashboard wire harness A 22P connector |  | O |  | 17, 18
C2 | Dashboard wire harness A 22P connector |  | O |  | 19, 20
C3 | Dashboard wire harness A 6P connector | O |  |  | 21
C4 | Floor wire harness 6P connector |  | O |  | 22

*1: The connector numbers are original in this section that are different from other sections.

*2: Note

a: Spring loaded lock connector

b: With built-in short contact connector

c: Waterproof connector