## Engine Assembly

#### Engine Installation

5-13

1. Install the accessory brackets and tighten their bolts and nuts to the specified torques.

   1. REAR STIFFENER

      (D15Y4,D17A2 engines M/T, HONDA MULTIMATIC)

   2. REAR STIFFENER

      (D17A2 engine A/T)

   3. P/S PUMP BRACKET (P/S)
   4. ENGINE MOUNT BRACKET
   5. A/C COMPRESSOR BRACKET
   6. STIFFENER

      (Except D15Y4, D17A1 engines)

   7. FRONT STIFFENER

      (D15Y4, D17A2 engines)