## Frame Repair Chart

#### Side View (cont'd)

4-11

m | Locate hole o 25 (0.98) | u | For upper arm bracket center o15 (0.59)
n | For trailing arm o 13 (0.51) | v1, v2 | Locate hole o 13 (0.51)
o | Locate hole o 25 (0.98) | w | For upper arm o 13 (0.51)
p | Locate hole o 20 (0.79) | x | For rear lower arm centre
q | Trailing arm centre | y | Locate hole o 50 (1.97)
r | Rear damper center 73 x 68 (slot) | z | Locate hole o 20 (0.79)
s | For upper arm o 13 (0.51)
t | For trailing arm o 13 (0.51)