## Sunroof

#### Drain Channel Replacement

20-196

1. Remove the glass (see page 20-194).

2. With the sunroof wrench, move both glass brackets (A) to the position where the sunroof normally pivots down and remove the screws securing the drain channel (B).

   Fastener Locations
   : Screw, 2

3. Release the drain channel (A) from both hooks (B) of the drain channel slider by pulling the drain channel forward.

4. Remove the drain channel (A).

5. Install the channel in the reverse order of removal and note these items:

- Push the drain channel onto the hooks until a faint click is heard.
- Check the glass height adjustment (see page 20-194).

6. Check for water leaks. Let the water run freely from a hose without a nozzle. Do not use a high-pressure spray.