## Opening Repair Chart

####

4-22

Door and Windshield Openings:

Unit: mm (in.)

1. A

   Windshield lower dashboard guide pin

2. B, C

   Windshield opening flange notch (3 places)

3. D, E, F, G, H, I, J, K,

   Door opening flange notch (16 places)

Tailgate Opening:

1. L

   Roof lower Rail Flange notch

2. M

   Rear Gutter Lower Stiffener flange end (2 places)

3. N

   Rear panel upper stiffener water drain notch