## Transmission End Cover

#### End Cover, 1st Gears and 1st Clutch Removal

14-172

Exploded View

1. END COVER GASKET

   Replace.

2. END COVER
3. TRANSMISSION RANGE SWITCH COVER
4. TRANSMISSION RANGE SWITCH
5. TRANSMISSION RANGE SWITCH HARNESS
6. HARNESS CLAMPS
7. PARK LEVER
8. COUNTERSHAFT

   Replace.

9. CONICAL SPRING WASHER

   Replace

10. PARK GEAR
11. ONE-WAY CLUTCH
12. COUNTERSHAFT 1ST GEAR
13. NEEDLE BEARING
14. COUNTERSHAFT 1ST GEAR COLLAR
15. SEALING WASHERS

    Replace.

16. LINE BOLT
17. ATF COOLER LINES
18. LINE BOLT
19. MAINSHAFT 1ST GEAR COLLAR
20. A/T CLUTCH PRESSURE CONTROL SOLENOID VALVES A and B
21. MAINSHAFT 1ST GEAR
22. NEEDLE BEARING
23. THRUST NEEDLE BEARING
24. THRUST WASHER
25. 1ST CLUTCH ASSEMBLY
26. CONICAL SPRING WASHER

    Replace.

27. MAINSHAFT LOCKNUT

    Replace.