## Power Windows

#### Master Switch Replacement

22-9

Passenger's Switch Replacement

1. Remove the door grip (see page 20-4).
2. Remove the power window master switch (A) from the door lining.

3. Disconnect the 14P connector (B) from the switch.
4. Remove the three screws and switch from the switch panel.

1. Remove the door grip (see page 20-4).
2. Remove the power window switch (A) from the door lining.

3. Disconnect the 5P connector (B) from the switch.
4. Remove the two screws and switch from the switch panel.

a a a